
**Product introduction**

**Array microphone NAJA A302**

With a dust-proof mesh cover, the use time is longer, and the pickup distance is 5-8Meter, directional broadband directivity, suitable for a variety of application scenarios, and can be adapted to other products of Soundfit to meet the needs.



**Main features**

★1. Overcurrent protection;

★2. High temperature protection;

★3. Overload protection;

4. Directional broadband directivity;

★5. Pickup distance: 5-8 meters;

★6. Frequency response: 20-18KHz;

★7. Signal-to-noise ratio: 80dB.

|  |  |
| --- | --- |
| Output Interface | 3pin Phoenix terminal balanced output |
| channel separation | 100dB |
| Directivity | Directional Broadband |
| Dynamic Range | 95dB |
| Number of microphones | 5 |
| Microphone type | Capacitor Microphone |
| Operating Voltage | 48V phantom power supply |
| Sensitivity | -10dB |
| Maximum power consumption | 1W |
| maximum boost stage | 113dB SPL@1kHZ |
| Frequency response | 20-18KHz |
| signal to noise ratio | 80dB |

**Product Specifications**